{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXF-A"]
[]
[]
[]
[]
["","","","","","2AMXF40A2V1B"]
["Méretek","Egység","","Magasság","mm","550"]
["","","","Szélesség","mm","765"]
["","","","Mélység","mm","285"]
["Tömeg","Egység","","","kg","36"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","500"]
["","","Fűtés","Szuper alacsony","1/perc","320"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10"]
["","","","Max.","°C száraz hőm.","46"]
["Hangnyomás szint","Hűtés","","Magas","dBA","46"]
["","Fűtés","","Magas","dBA","48"]
["Hűtőközeg","Típus","","","","R-32"]
["","Töltet","","","kg","0.88"]
["","Töltet","","","tCO2Eq","0.60"]
["","GWP","","","","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (20m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15.0"]
["","","IU - IU","Max.","m","7.5"]
["","Összes csőhossz","Rendszer","Aktuális","m","30"]
["Standard Accessories","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Screw bag","","","","1"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-230-240"]
["Notes","","","","","(1) - Egy helyiséghez"]