{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM40M2V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","","","30","34"]
["","","Fűtés","Szuper alacsony","m³/perc","","","32","34"]
["Hangteljesítményszint","Fűtés","","","dB(A)","","62","","","62"]
["","Hűtés","","","dB(A)","","60","","","60"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","cfm","","","1059","1200"]
["","","Fűtés","Szuper alacsony","cfm","","","1130","1200"]
["Méretek","Egység","","Magasság","mm","550","550","550","550","550","550"]
["","","","Szélesség","mm","765","765","765","765","765","765"]
["","","","Mélység","mm","285","285","285","285","285","285"]
["Tömeg","Egység","","","kg","36","36","36","41","41","41"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","500","500","760","890","500","500"]
["","","Fűtés","Szuper alacsony","1/perc","320","320","820","890","500","500"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","","46.0","-10","-10","46.0"]
["","","","Max.","°C száraz hőm.","","-10","46","46","-10"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","","-15","-15","-15","-15.0"]
["","","","Max.","°C párás hőm.","","18.0","18","18","18.0"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","46","46","","","48","48"]
["","","","Névl.","dB(A)","","","48","46"]
["","Fűtés","","Magas","dB(A)","48","48","","","50","50"]
["","","","Névl.","dB(A)","","","50","48"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Töltet","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Töltet","","","tCO2Eq","0.59","0.6","0.6","0.8","0.78","0.78"]
["","GWP","","","","675.0","675","675","675","675","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20","20 (1)","20","20","20 (1)","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)","002 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15.0","15","15","15","15","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Összes csőhossz","Rendszer","Aktuális","m","30","30","30","30","30","30"]
["Standard Accessories","Installation manual","","","","1","1","Installation manual","1","1","1"]
["","Drain plug","","","","1","1","Drain plug","1","1","1"]
["","Screw bag","","","","1","1","Screw bag","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","50"]
["","Feszültség","","","V","220-230-240","220-230-240","220-240","220-240","220-230-240","220-230-240"]
["Notes","","","","","(1) - Egy helyiséghez","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","","","(1) - Egy helyiséghez"]
["","","","","","","(1) - Egy helyiséghez","","","(1) - Egy helyiséghez"]
["","","","","","","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát","","","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","","(3) - Az elektromos adatokat lásd külön rajzokon","","","(3) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","","","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Kompresszor","Típus","","","","","","Hermetikusan zárt lengő kompresszor"]
["Standard Accessories","Reducer assembly","","","","","","","1","1","1"]