{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M"]
[]
[]
[]
[]
["","","","","","2MXM40M2V1B","2MXM40M4V1B","2MXM40M3V1B","2MXM50M2V1B"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","30","","","34"]
["","","Fűtés","Szuper alacsony","m³/perc","32","","","34"]
["","","","Szuper alacsony","cfm","1059","","","1200"]
["","","Fűtés","Szuper alacsony","cfm","1130","","","1200"]
["Méretek","Egység","","Magasság","pp","550","550","550","550"]
["","","","Szélesség","pp","765","765","765","765"]
["","","","Mélység","pp","285","285","285","285"]
["Tömeg","Egység","","","kg","36","36","36","41"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","760","500","500","890"]
["","","Fűtés","Szuper alacsony","1/perc","820","320","320","890"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10","-10 (2)","-10"]
["","","","Max.","°C száraz hőm.","46","46","46 (2)","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15","-15","-15","-15"]
["","","","Max.","°C párás hőm.","18","18","18","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","46","46"]
["","","","Névl.","dB(A)","48","","","46"]
["","Fűtés","","Magas","dB(A)","","48","48"]
["","","","Névl.","dB(A)","50","","","48"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32","R-32"]
["","Töltet","","","kg","0.88","0.88","0.88","1.15"]
["","Töltet","","","tCO2Eq","0.6","0.60","0.59","0.8"]
["","GWP","","","","675","675","675","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20","20","20 (1)","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15","15.0","15.0","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5"]
["","Összes csőhossz","Rendszer","Aktuális","m","30","30","30","30"]
["Standard Accessories","Installation manual","","","","Installation manual","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","220-240","220-230-240","220-230-240","220-240"]
["Notes","","","","","","(1) - Egy helyiséghez"]
["","","","","","","","(1) - Egy helyiséghez"]
["","","","","","","","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["Standard Accessories","Reducer assembly","","","","","","","1"]