{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Méretek","Egység","","Magasság","mm","550","550","734"]
["","","","Szélesség","mm","765","765","958"]
["","","","Mélység","mm","285","285","340"]
["Tömeg","Egység","","","kg","36","41","60"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","500","500","420"]
["","","Fűtés","Szuper alacsony","1/perc","320","500","420"]
["Kompresszor","Type","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","","","-10"]
["","","","Max.","°C száraz hőm.","","","46"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","46","48"]
["","","","Névl.","dB(A)","","","48"]
["","Fűtés","","Magas","dB(A)","48","50"]
["","","","Névl.","dB(A)","","","48.0"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32"]
["","Töltet","","","kg","0.88","1.15","2"]
["","Töltet","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20","20","25"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (30m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15.0","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Összes csőhossz","Rendszer","Aktuális","m","30","30","50"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-230-240","220-230-240","220-240"]
["Notes","","","","","(1) - Egy helyiséghez","(1) - Egy helyiséghez","(1) - Egy helyiséghez"]
["Standard Accessories","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]