{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","48","48","","50","50"]
["","Hűtés","","Névl.","dB(A)","47","47","","48","48"]
["Standard Accessories","Telepítési utasítás","","","","1","1","","1","1"]
["","Csavarzsák","","","","1","1","","1","1"]
["","Leeresztő csavar","","","","1","1","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Feltöltés","","","kg","1.20","1.20","","1.60","1.60"]
["","Típus","","","","R-410A","R-410A","","R-410A","R-410A"]
["Csőcsatlakozások","Szintkülönbség","IU - IU","Max.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Max.","m","15","15","","15","15"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)","","0,02 (20m-t meghaladó csőhosszhoz)","0,02 (20m-t meghaladó csőhosszhoz)"]
["","Összes csőhossz","Rendszer","Aktuális","m","30","30","","30","30"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Méretek","Egység","","Szélesség","mm","765","765","","765","765"]
["","","","Mélység","mm","285","285","","285","285"]
["","","","Magasság","mm","550","550","","550","550"]
["Tömeg","Egység","","","kg","38","38","","42","42"]
["Power supply","fázis","","","","1~","1~","","1~","1~"]
["","Frekvencia","","","Hz","50","50","","50","50"]
["","Feszültség","","","V","220-240","220-240","","220-240","220-240"]
["Notes","","","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Méretek","Egység","","Magasság","mm","","","550","","","550"]
["","","","Szélesség","mm","","","765","","","765"]
["","","","Mélység","mm","","","285","","","285"]
["Tömeg","Egység","","","kg","","","38","","","42"]
["Kompresszor","Típus","","","","","","Hermetikusan zárt lengő kompresszor","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","","","10","","","10"]
["","","","Max.","°C száraz hőm.","","","46","","","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","","","-15","","","-15"]
["","","","Max.","°C párás hőm.","","","15.5","","","15.5"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","","","47","","","48"]
["","Fűtés","","Névl.","dB(A)","","","48","","","50"]
["Hűtőközeg","Típus","","","","","","R-410A","","","R-410A"]
["","Töltet","","","kg","","","1.20","","","1.60"]
["","Töltet","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","","","20","","","20"]
["","További hűtőközeg utántöltés","","","kg/m","","","0,02 (20m-t meghaladó csőhosszhoz)","","","0,02 (20m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","","","15","","","15"]
["","","IU - IU","Max.","m","","","7.5","","","7.5"]
["","Összes csőhossz","Rendszer","Aktuális","m","","","30","","","30"]
["Standard Accessories","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Áramellátás","fázis","","","","","","1~","","","1~"]
["","Frekvencia","","","Hz","","","50","","","50"]
["","Feszültség","","","V","","","220-240","","","220-240"]
["Standard Accessories","Nyomáscsökkentő szelep szerelvény","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]