{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B","3MXM52N2V1B","3MXM68N2V1B"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","24","24","24.1"]
["","","Fűtés","Szuper alacsony","m³/perc","24","24","24.1"]
["","","","Szuper alacsony","cfm","847","847","851"]
["","","Fűtés","Szuper alacsony","cfm","847","847","851"]
["Méretek","Egység","","Magasság","pp","734","734","734"]
["","","","Szélesség","pp","958","958","958"]
["","","","Mélység","pp","340","340","340"]
["Tömeg","Egység","","","kg","57","57","62"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","420","420"]
["","","Fűtés","Szuper alacsony","1/perc","420","420"]
["Kompresszor","Type","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10","-10"]
["","","","Max.","°C száraz hőm.","46","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15","-15","-15"]
["","","","Max.","°C párás hőm.","18","18","18"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","46","46","48"]
["","Fűtés","","Névl.","dB(A)","47","47","48"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32"]
["","Töltet","","","kg","1.80","1.80","2.00"]
["","Töltet","","","tCO2Eq","1.2","1.2","1.4"]
["","GWP","","","","675","675","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","25","25","25"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (30m-t meghaladó csőhosszhoz)","0,02 (30m-t meghaladó csőhosszhoz)","0,02 (30m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15","15","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Összes csőhossz","Rendszer","Aktuális","m","50","50","50"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]
["Standard Accessories","Drain cap","","","","","","3"]
["","Reducer assembly","","","","","","1"]