{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-K"]
[]
[]
[]
[]
["","","","","","3MXS40K3V1B","3MXS40K3V1B2","3MXS40K2V1B"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","47","47"]
["","Hűtés","","Névl.","dB(A)","46","46"]
["Standard Accessories","Telepítési utasítás","","","","1","1"]
["","Leeresztő csavar","","","","1","1"]
["Hűtőközeg","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","2.0","2.0"]
["","Típus","","","","R-410A","R-410A"]
["Csőcsatlakozások","Szintkülönbség","IU - IU","Max.","m","7.5","7.5"]
["","","IU - OU","Max.","m","15","15"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (30m-t meghaladó csőhosszhoz)","0,02 (30m-t meghaladó csőhosszhoz)"]
["","Összes csőhossz","Rendszer","Aktuális","m","50","50"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Méretek","Egység","","Szélesség","mm","936","936"]
["","","","Mélység","mm","300","300"]
["","","","Magasság","mm","735","735"]
["Tömeg","Egység","","","kg","49","49"]
["Power supply","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","230","230"]
["Notes","","","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Méretek","Egység","","Magasság","mm","","","735"]
["","","","Szélesség","mm","","","936"]
["","","","Mélység","mm","","","300"]
["Tömeg","Egység","","","kg","","","49"]
["Kompresszor","Típus","","","","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","","","-10"]
["","","","Max.","°C száraz hőm.","","","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","","","-15"]
["","","","Max.","°C párás hőm.","","","15.5"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","","","46"]
["","Fűtés","","Névl.","dB(A)","","","47"]
["Hűtőközeg","Típus","","","","","","R-410A"]
["","Töltet","","","kg","","","2.0"]
["","Töltet","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","","","50"]
["","További hűtőközeg utántöltés","","","kg/m","","","0,02 (30m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["Standard Accessories","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["Áramellátás","fázis","","","","","","1~"]
["","Frekvencia","","","Hz","","","50"]
["","Feszültség","","","V","","","230"]