{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Méretek","Egység","","Magasság","mm","734","734"]
["","","","Szélesség","mm","1040","1040"]
["","","","Mélység","mm","408","408"]
["Tömeg","Egység","","","kg","69","73"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10"]
["","","","Max.","°C száraz hőm.","46","46"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","48","52"]
["","Fűtés","","Névl.","dB(A)","49","53"]
["Hűtőközeg","Típus","","","","R-32","R-32"]
["","Töltet","","","kg","2","2.4"]
["","Töltet","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","25 (2)","25 (3)"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (30m-t meghaladó csőhosszhoz)","0,02 (30m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15 (3)","15"]
["","","IU - IU","Max.","m","7.5 (3)","7.5 (3)"]
["","Összes csőhossz","Rendszer","Aktuális","m","60","75"]
["Standard Accessories","Telepítési utasítás","","","","1","1"]
["","Leeresztő sapka","","","","3","3"]
["","Leeresztő csavar","","","","1","1"]
["","Nyomáscsökkentő szelep szerelvény","","","","1","1"]
["","Csavarzsák","","","","2","2"]
["Energiatakarékossági besorolás","","","","","A+++ ~ D","A+++ ~ D"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-440","220-240"]
["Notes","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(2) - Egy helyiséghez","(2) - Egy helyiséghez"]
["","","","","","(3) - Egy helyiségbe (FBA71/100/125 és EKHWET és CKHWS egységekkel történő kombináláskor hivatkozzon a telepítési útmutatóra)","(3) - Egy helyiségbe (FBA71/100/125 és EKHWET és CKHWS egységekkel történő kombináláskor hivatkozzon a telepítési útmutatóra)"]
["","","","","","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]