{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":6,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-A8"]
[]
[]
[]
[]
["","","","","","5MXM90A2V1B8"]
["Méretek","Egység","","Magasság","mm","734"]
["","","","Szélesség","mm","974"]
["","","","Mélység","mm","408"]
["Tömeg","Egység","","","kg","68"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10"]
["","","","Max.","°C száraz hőm.","50"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","52"]
["","Fűtés","","Névl.","dB(A)","52"]
["Hűtőközeg","Típus","","","","R-32"]
["","Töltet","","","kg","2.40"]
["","Töltet","","","tCO2Eq","1.62"]
["","GWP","","","","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","25 (1)"]
["","További hűtőközeg utántöltés","","","kg/m","002 (30m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Összes csőhossz","Rendszer","Aktuális","m","75"]
["Standard Accessories","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]
["Notes","","","","","(1) - Egy helyiséghez"]
["","","","","","(2) - A CVXM-A, FVXM-A egységekkel kombinálva – a maximális csőhossz 30m."]
["","","","","","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(4) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","(5) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]