{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Méretek","Egység","","Magasság","mm","734","734"]
["","","","Szélesség","mm","1040","1040"]
["","","","Mélység","mm","408","408"]
["Tömeg","Egység","","","kg","69.0","73.0"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10"]
["","","","Max.","°C száraz hőm.","50","50"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","48.0 (2)","52.0 (2)"]
["","Fűtés","","Névl.","dB(A)","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Hűtőközeg","Típus","","","","R-32","R-32"]
["","Töltet","","","kg","2.00","2.40"]
["","Töltet","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675.0"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","25 (4) (5)","25 (5) (4)"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (30m-t meghaladó csőhosszhoz)","0,02 (30m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15.0 (5)","15.0 (5)"]
["","","IU - IU","Max.","m","7.5 (5)","7.5 (5)"]
["","Összes csőhossz","Rendszer","Aktuális","m","60","75"]
["Standard Accessories","Telepítési utasítás","","","","1","1"]
["","Leeresztő sapka","","","","3","3"]
["","Leeresztő csavar","","","","1","1"]
["","Nyomáscsökkentő szelep szerelvény","","","","1","1"]
["","Csavarzsák","","","","2","2"]
["Energiatakarékossági besorolás","","","","","A+++ ~ D","A+++ ~ D"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]
["Notes","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrákat","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrákat"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - Egy helyiséghez","(4) - Egy helyiséghez"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(6) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]