{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standard Accessories","Telepítési utasítás","","","","Telepítési utasítás"]
["","Használati utasítás","","","","Használati utasítás"]
["","Csavar+alátét","","","","Csavar+alátét"]
["","Vezeték nélküli távirányító","","","","Vezeték nélküli távirányító"]
["","Burkolatzáró rács","","","","Burkolatzáró rács"]
["","Akkumulátor","","","","Akkumulátor"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","9.52"]
["","Gáz","","Külső átm.","pp","15.88"]
["","Ürítés","","","","19.05"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.128"]
["","Fűtés","","Névl.","kW","0.128"]
["Sound power level","Hűtés","","","dB(A)","64"]
["","Fűtés","","","dB(A)","64"]
["Méretek","Egység","","Szélesség","pp","600"]
["","","","Mélység","pp","1,007"]
["","","","Magasság","pp","285"]
["Burkolat","Anyag","","","","Galvanizált acél"]
["Tömeg","Egység","","","kg","35"]
["Ventilátor","Külső statikus nyomás","","Magas","Pa","90"]
["","","","Névl.","Pa","77"]
["","","","Alacsony","Pa","64"]
["Power supply","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Megnevezés","","","","V1"]
["","Feszültség","","","V","220-240"]
["Elektromos bemenet","Fűtés","","Névl.","kW","","0.109"]
["","Hűtés","","Névl.","kW","","0.109"]
["Ventilátor","Külső statikus nyomás","","Magas","Pa","","70","150","150"]
["","","","Alacsony","Pa","","45","111","92"]
["Burkolat","Anyag","","","","","Galvanizált acél"]
["Méretek","Egység","","Magasság","pp","","378","378","378"]
["","","","Szélesség","pp","","541","1300","1500"]
["","","","Mélység","pp","","1045","541","541"]
["Tömeg","Egység","","","kg","","44","50","56"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","22.7","40.5","48.7"]
["","","","Névl.","m³/perc","","20.5","37","44"]
["","","","Alacsony","m³/perc","","18.3","34.8","37.9"]
["","","Fűtés","Magas","m³/perc","","22.7","40.5","48.7"]
["","","","Névl.","m³/perc","","20.5","37.4","43.9"]
["","","","Alacsony","m³/perc","","18.3","34.8","37.9"]
["","Külső statikus nyomás","","Névl.","Pa","","57","128","122"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","60","72","73"]
["","Fűtés","","","dB(A)","","60","72","73"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","41","53","55"]
["","","","Névl.","dB(A)","","38"]
["","","","Alacsony","dB(A)","","36","50","50"]
["","Fűtés","","Magas","dB(A)","","41","53","55"]
["","","","Névl.","dB(A)","","38"]
["","","","Alacsony","dB(A)","","36","50","50"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","pp","","15.88","15.9","15.9"]
["","Ürítés","","","","","19.05"]
["Standard Accessories","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Áramellátás","fázis","","","","","1~"]
["","Frekvencia","","","Hz","","50"]
["","Feszültség","","","V","","220-240"]
["Hűtési teljesítmény","Hűtési összteljesítmény","","Névl.","kW","","","12.10","13.00"]
["Fűtési teljesítmény","Összes teljesítmény","","Névl.","kW","","","13.5","15.5"]
["Burkolat","Szín","","","","","","Galvanizált acél lemez / Festés nélkül","Galvanizált acél lemez / Festés nélkül"]
["Ventilátor","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","","37","44"]
["","","Fűtés","Közepes","m³/perc","","","37.4","43.9"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","","52","53"]
["","Fűtés","","Közepes","dB(A)","","","52","53"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","","ARCWLA","ARCWLA"]