{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","","44","","47"]
["","","","Névl.","dB(A)","","41","","44"]
["","","","Csendes működés","dB(A)","","36","","41"]
["","","","Alacsony","dB(A)","","38","","43"]
["","Hűtés","","Csendes működés","dB(A)","","36","","41"]
["","","","Alacsony","dB(A)","","38","","43"]
["","","","Magas","dB(A)","","44","","47"]
["","","","Névl.","dB(A)","","41","","44"]
["Standard Accessories","Telepítési utasítás","","","","","Telepítési utasítás","","Telepítési utasítás"]
["","Használati utasítás","","","","","Használati utasítás","","Használati utasítás"]
["","Csavarok","","","","","Csavarok","","Csavarok"]
["","Alátét","","","","","Alátét","","Alátét"]
["","Vezeték nélküli távirányító","","","","","Vezeték nélküli távirányító","","Vezeték nélküli távirányító"]
["","Burkolatzáró rács","","","","","Burkolatzáró rács","","Burkolatzáró rács"]
["","Akkumulátor","","","","","Akkumulátor","","Akkumulátor"]
["Vezérlőrendszerek","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Folyadék","","Külső átm.","mm","","9.52","","9.52"]
["","Gáz","","Külső átm.","mm","","15.88","","15.88"]
["","Ürítés","","","","","19.05","","19.05"]
["Áramfelvétel","Hűtés","","Névl.","kW","","0.094","","0.137"]
["","Fűtés","","Névl.","kW","","0.094","","0.137"]
["Hangteljesítmény szintje","Hűtés","","","dB(A)","","56","","60"]
["","Fűtés","","","dB(A)","","56","","60"]
["Méretek","Berendezés","","Szélesség","mm","","820","","820"]
["","","","Mélység","mm","","820","","820"]
["","","","Magasság","mm","","300","","300"]
["Burkolat","Anyag","","","","","Galvanizált acél","","Galvanizált acél"]
["Tömeg","Egység","","","kg","","39","","39"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","","29.2","","34.0"]
["","","","Alacsony","m³/perc","","21.0","","26.3"]
["","","","Névl.","m³/perc","","24.4","","29.2"]
["","","Hűtés","Alacsony","m³/perc","","21.0","","26.3"]
["","","","Névl.","m³/perc","","24.4","","29.2"]
["","","","Magas","m³/perc","","29.2","","34.0"]
["","","","Csendes működés","m³/perc","","17.6","","22.1"]
["","","Hűtés","Csendes működés","m³/perc","","17.6","","22.1"]
["Dekorációs panel","Tömeg","","","kg","","4","","4"]
["","Méretek","","Magasság","mm","","82","","82"]
["","","","Mélység","mm","","990","","990"]
["","","","Szélesség","mm","","990","","990"]
["","Szín","","","","","Fehér","","Fehér"]
["Power supply","Phase","","","","","1~","","1~"]
["","Megnevezés","","","","","V1","","V1"]
["","Frekvencia","","","Hz","","50","","50"]
["","Feszültség","","","V","","220-240","","220-240"]
["Ventilátor","Légáramlási arány","Fűtés","Csendes működés","m³/perc","15","","22.1"]
["Elektromos bemenet","Fűtés","","Névl.","kW","0.067","","0.137"]
["","Hűtés","","Névl.","kW","0.067","","0.137"]
["Ventilátor","Légáramlási arány","Hűtés","Csendes működés","m³/perc","15","","22.1"]
["Burkolat","Anyag","","","","Galvanizált acél","","Galvanizált acél"]
["Méretek","Egység","","Magasság","mm","265","","300"]
["","","","Szélesség","mm","820","","820"]
["","","","Mélység","mm","820","","820"]
["Tömeg","Egység","","","kg","31","","39"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","24.4","","34"]
["","","","Névl.","m³/perc","20.5","","29.2"]
["","","","Alacsony","m³/perc","17.6","","26.3"]
["","","Fűtés","Magas","m³/perc","24.4","","34"]
["","","","Névl.","m³/perc","20.5","","29.2"]
["","","","Alacsony","m³/perc","17.6","","26.3"]
["Hangteljesítményszint","Hűtés","","","dB(A)","54","","60"]
["","Fűtés","","","dB(A)","54","","60"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","41","","47"]
["","","","Névl.","dB(A)","38","","44"]
["","","","Alacsony","dB(A)","35","","43"]
["","","","Csendes működés","dB(A)","32","","41"]
["","Fűtés","","Magas","dB(A)","41","","47"]
["","","","Névl.","dB(A)","38","","44"]
["","","","Alacsony","dB(A)","35","","43"]
["","","","Csendes működés","dB(A)","32","","41"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","9.52","","9.52"]
["","Gáz","","Külső átm.","mm","15.88","","15.88"]
["","Ürítés","","","","19.05","","19.05"]
["Dekorációs panel","Méretek","","Magasság","mm","82","","82"]
["","","","Szélesség","mm","990","","990"]
["","","","Mélység","mm","990","","990"]
["","Tömeg","","","kg","4","","4"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARCWLA","","ARCWLA"]
["","Vezetékes távszabályzó","","","","ARCWB","","ARCWB"]
["Standard Accessories","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Áramellátás","fázis","","","","1~","","1~"]
["","Frekvencia","","","Hz","50","","50"]
["","Feszültség","","","V","220-240","","220-240"]