{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":11,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA35A2VEB","ADEA50A2VEB","ADEA60A2VEB","ADEA71A2VEB","ADEA100A2VEB","ADEA125A2VEB"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","37","37","31"]
["","","","Közepes","dB(A)","34","34","28"]
["","","","Alacsony","dB(A)","29","29","25"]
["","Hűtés","","Közepes","dB(A)","32","32","28"]
["","","","Alacsony","dB(A)","29","29","25"]
["","","","Magas","dB(A)","35","35","30"]
["Standard Accessories","Használati utasítás","","","","1","1","1"]
["","Telepítési utasítás","","","","1","1","1"]
["","Leeresztő tömlő","","","","1","1","1"]
["","Az leeresztő tömlő fémbilincse","","","","1","1","1"]
["","Alátét a függesztőkerethez","","","","8","8","8"]
["","Csavarok","","","","40","40","40"]
["","Szigetelés a szereléshez","","","","2","2","2"]
["","Tömítések","","","","5","5","5"]
["","Bilincsek","","","","4","4","4"]
["Vezérlőrendszerek","Wired remote control","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.52","12.70","12.70"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Hangteljesítmény szintje","Hűtés","","","dB(A)","60","60","56"]
["Méretek","Berendezés","","Szélesség","mm","700","700","1,000"]
["","","","Mélység","mm","800","800","800"]
["","","","Magasság","mm","245","245","245"]
["Burkolat","Anyag","","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["","Colour","","","","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)"]
["Tömeg","Egység","","","kg","28.0","28.0","35.0"]
["Ventilátor","Külső statikus nyomás","","Magas","Pa","150","150","150"]
["","","","Névl.","Pa","30","30","30"]
["","Légáramlási arány","Fűtés","Magas","m³/perc","15.0","15.0","18.0"]
["","","","Alacsony","m³/perc","10.5","10.5","12.5"]
["","","","Medium","m³/perc","12.5","12.5","15.0"]
["","","Hűtés","Alacsony","m³/perc","10.5","10.5","12.5"]
["","","","Medium","m³/perc","12.5","12.5","15.0"]
["","","","Magas","m³/perc","15.0","15.0","18.0"]
["Leeresztési emelési magasság","mm","","","","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - Az hangteljesítmény szintje a hangforrás által keltett abszolút érték.","(1) - Az hangteljesítmény szintje a hangforrás által keltett abszolút érték.","(1) - Az hangteljesítmény szintje a hangforrás által keltett abszolút érték.","(1) - Az hangteljesítmény szintje a hangforrás által keltett abszolút érték.","(1) - Az hangteljesítmény szintje a hangforrás által keltett abszolút érték.","(1) - Az hangteljesítmény szintje a hangforrás által keltett abszolút érték."]
["","","","","","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon"]
["Ventilátor","Külső statikus nyomás","","Magas","Pa","","","","150","150","150"]
["Burkolat","Szín","","","","","","","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)"]
["","Anyag","","","","","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["Méretek","Egység","","Magasság","mm","","","","245","245","245"]
["","","","Szélesség","mm","","","","1000","1400","1400"]
["","","","Mélység","mm","","","","800","800","800"]
["Tömeg","Egység","","","kg","","","","35","46","46"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","","","18","29","34"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","","","15","26","29"]
["","","","Alacsony","m³/perc","","","","12.5","23","23.5"]
["","","Fűtés","Magas","m³/perc","","","","18","29","34"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","","","15","26","29"]
["","","Fűtés","Alacsony","m³/perc","","","","12.5","23","23.5"]
["","Külső statikus nyomás","","Névl.","Pa","","","","30","40","50"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","","","56","58","62"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","","","30","34","37"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","","","28","32","35"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","","","25","30","32"]
["","Fűtés","","Magas","dB(A)","","","","31","36","38"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","","","28","33","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","","","","25","30","32"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","","","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","mm","","","","15.9","15.9","15.9"]
["","Ürítés","","","","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Leeresztési emelési magasság","mm","","","","","","","625","625","625"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Vezetékes távszabályzó","","","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Installation manual","","","","","","","1","1","1"]
["","Washer for hanger bracket","","","","","","","8","8","8"]
["","Operation manual","","","","","","","1","1","1"]
["","Clamps","","","","","","","4","4","4"]
["","Drain hose","","","","","","","1","1","1"]
["","Insulation for fitting","","","","","","","2","2","2"]
["","Metal clamp for drain hose","","","","","","","1","1","1"]
["","Screws","","","","","","","40","40","40"]
["","Sealing pads","","","","","","","5","5","5"]
["Áramellátás","fázis","","","","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","","","","50","50","50"]
["","Feszültség","","","V","","","","220-240/220","220-240/220","220-240/220"]
["Hűtési teljesítmény","Hűtési összteljesítmény","","Névl.","kW","","","","","","14.00"]
["Fűtési teljesítmény","Összes teljesítmény","","Névl.","kW","","","","","","13.50"]