{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEQ100A7VEB / AZQS100B8V1B","ADEQ125A7VEB / AZQS125B8V1B","ADEQ71A7VEB / AZQS71B2V1B (Archived)"]
["Hűtési teljesítmény","Névl.","","kW","9.5","12.1","6.8"]
["Felülethűtés","SEER","","","4.81","","4.81"]
["","Éves energiafogyasztás","","kWh/a","692","","494.77"]
["","Kapacitás","Pdesign","kW","9.50","","6.80"]
["","Energiatakarékossági osztály","","","B","","B"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","7.60","","6.00"]
["","SCOP/A","","","3.81","","3.81"]
["","Energiatakarékossági osztály","","","A","","A"]
["","Éves energiafogyasztás","","kWh/a","2,793","","2,205.68"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","1,480","2,010","1,060"]
["","EER","","","3.21","3.01","3.21"]
["","COP","","","3.61","3.45","3.61"]
["","Energiacímkézés irányelve","Hűtés","","A","","A"]
["","","Fűtés","","A","","A"]
["Fűtőkapacitás","Névl.","","kW","10.8","13.50","7.50"]
["Notes","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]