{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / ARXS-L3"]
[]
[]
[]
[]
["","","","ADEQ35C2VEB / ARXS35L3V1B"]
["Hűtési teljesítmény","Névl.","kW","3.40 (1)"]
["Fűtőkapacitás","Névl.","kW","4.00 (1)"]
["Notes","","","(1) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]
["","","","(2) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","(3) - PED: szerelvény = I. kategória : a 97/23/EK 3.6 fejezet 1. cikkelye alapján nem tartozik a PED kategóriába"]
["","","","(4) - Minimum Ssc (=Rövidzárlati teljesítmény) értéke: A berendezés megfelel az EN 61000-3-2 szabványnak"]
["","","","(5) - Az elektromos adatokat lásd külön rajzokon"]
["","","","(6) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]