{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","37","37","31","31","36","38"]
["","","Névl.","dB(A)","37","37","31","31","36","38"]
["","","Közepes","dB(A)","34","34","28","28","33","35"]
["","","Alacsony","dB(A)","29","29","25","25","30","32"]
["","Hűtés","Közepes","dB(A)","32","32","28","28","32","35"]
["","","Alacsony","dB(A)","29","29","25","25","30","32"]
["","","Magas","dB(A)","35","35","30","30","34","37"]
["","","Névl.","dB(A)","35","35","30","30","34","37"]
["Standard Accessories","Használati utasítás","","","1","1","1","1","1","1"]
["","Telepítési utasítás","","","1","1","1","1","1","1"]
["","Leeresztő tömlő","","","1","1","1","1","1","1"]
["","Az leeresztő tömlő fémbilincse","","","1","1","1","1","1","1"]
["","Alátét a függesztőkerethez","","","8","8","8","8","8","8"]
["","Csavarok","","","40","40","40","40","40","40"]
["","Szigetelés a szereléshez","","","2","2","2","2","2","2"]
["","Tömítőlemez","","","5","5","5","5","5","5"]
["","Bilincsek","","","4","4","4","4","4","4"]
["Hűtőközeg","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Hűtési teljesítmény","Összes teljesítmény","Névl.","kW","","","","","","12.10"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gáz","Külső átm.","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Ürítés","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Hűtés","","dB(A)","60","60","56","56","58","62"]
["Méretek","Egység","Szélesség","mm","700","700","1,000","1,000","1,400","1,400"]
["","","Mélység","mm","800","800","800","800","800","800"]
["","","Magasság","mm","245","245","245","245","245","245"]
["Casing","Material","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["","Colour","","","Festetlen","Festetlen","Festetlen","Festetlen","Festetlen","Festetlen"]
["Tömeg","Egység","","kg","28.0","28.0","35.0","35","46","46"]
["Ventilátor","Külső statikus nyomás","Magas","Pa","150","150","150","150","150","150"]
["","","Névl.","Pa","30","30","30","30","40","50"]
["Fűtőkapacitás","Összes teljesítmény","Névl.","kW","","","","","","13.5"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","Hz","50","50","50","50","50","50"]
["","Feszültség","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték."]