{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Elektromos bemenet","Fűtés","","Névl.","kW","0.106","0.149"]
["","Hűtés","","Névl.","kW","0.106","0.149"]
["Ventilátor","Külső statikus nyomás","","Magas","Pa","0","0","0","0"]
["","","","Alacsony","Pa","0","0","0","0"]
["Hűtési teljesítmény","Hűtési összteljesítmény","","Névl.","kW","","","12.10","13.00"]
["Fűtési teljesítmény","Összes teljesítmény","","Névl.","kW","","","13.5","15.5"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér","Fehér"]
["","Anyag","","","","Galvanizált acél","Galvanizált acél"]
["Méretek","Egység","","Magasság","pp","260","260","260","285"]
["","","","Szélesség","pp","1320","1538","1790","1900"]
["","","","Mélység","pp","634","634","634","680"]
["Tömeg","Egység","","","kg","38","45","65","70"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","23.8","31.1","34.4","43.9"]
["","","","Névl.","m³/perc","21.3","27.8","31","39"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","","31","39"]
["","","","Alacsony","m³/perc","18.9","24.8","27.2","28.3"]
["","","Fűtés","Magas","m³/perc","23.8","31.1","34.4","43.9"]
["","","","Névl.","m³/perc","21.3","27.8","30.6","39.1"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","","30.6","39.1"]
["","","Fűtés","Alacsony","m³/perc","18.9","24.8","27.2","28.3"]
["","Külső statikus nyomás","","Névl.","Pa","0","0","0","0"]
["Hangteljesítményszint","Hűtés","","","dB(A)","59","64","65","71"]
["","Fűtés","","","dB(A)","62","64","65","71"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","49","52","52","56"]
["","","","Névl.","dB(A)","48","47"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","","50","53"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","46","46","49","46"]
["","Fűtés","","Magas","dB(A)","49","52","52","56"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","","50","53"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","48","47"]
["","","","Alacsony","dB(A)","46","46","49","46"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","9.52","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","pp","15.88","15.88","15.9","15.9"]
["","Ürítés","","","","19.05","19.05"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Vezetékes távszabályzó","","","","ARCWB","ARCWB"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Leeresztőcső","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]