{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXB-C"]
[]
[]
[]
[]
["","","","","","ARXB25C2V1B","ARXB25C5V1B9","ARXB35C2V1B","ARXB35C5V1B9","ARXB50CV1B","ARXB60CV1B"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","","","","","51"]
["","Hűtés","","Névl.","dB(A)","","","","","51"]
["Refrigerant","Charge","","","TCO2Eq","","","","","3.0"]
["","GWP","","","","","","","","2,087.5"]
["","Charge","","","kg","","","","","1.45"]
["","Típus","","","","","","","","R-410A"]
["Compressor","Típus","","","","","","","","Hermetikus légterelő"]
["Méretek","Egység","","Szélesség","mm","","","","","855"]
["","","","Mélység","mm","","","","","328"]
["","","","Magasság","mm","","","","","753"]
["Tömeg","Egység","","","kg","","","","","44"]
["Áramellátás","fázis","","","","","","","","1~"]
["","Frekvencia","","","Hz","","","","","50"]
["","Feszültség","","","V","","","","","220-240"]
["Notes","","","","","","","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Méretek","Egység","","Magasság","mm","550","550","550","550","","753"]
["","","","Szélesség","mm","658","658","658","658","","855"]
["","","","Mélység","mm","275","275","275","275","","328"]
["Tömeg","Egység","","","kg","28","26","30","28","","44"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","","Hermetikus légterelő"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10","-10","-10","","-10"]
["","","","Max.","°C száraz hőm.","46","46","46","46","","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15","-15","-15","-15","","-15"]
["","","","Max.","°C párás hőm.","18","18","18","18","","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","46","46","48","48"]
["","Fűtés","","Magas","dB(A)","47","47","48","48"]
["Hűtőközeg","Típus","","","","R-410A","R-410A","R-410A","R-410A","","R-410A"]
["","Töltet","","","kg","0.74","0.74","1.0","1.0","","1.45"]
["","Töltet","","","tCO2Eq","1.5","1.5","2.1","2.1","","3.0"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","","2087.5"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","","1~"]
["","Frekvencia","","","Hz","50","50","50","50","","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240","","220-240"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","","15","","15","","30"]
["","További hűtőközeg utántöltés","","","kg/m","","0,02 (10m-t meghaladó csőhosszhoz)","","0,02 (10m-t meghaladó csőhosszhoz)"]
["Standard Accessories","LOT10 Energy Label","","","","","LOT10 Energy Label","","LOT10 Energy Label"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","","","","","","51"]
["","Fűtés","","Névl.","dB(A)","","","","","","51"]