{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","","49.0"]
["","Hűtés","","Névl.","dB(A)","","49.0"]
["Standard Accessories","Leeresztő csavar","","","","","1"]
["","Telepítési utasítás","","","","","1"]
["","Hűtőközeg töltési címke","","","","","1"]
["","Fluorinált káros gázokra vonatkozó többnyelvű címke","","","","","1"]
["","Általános biztonsági óvintézkedések","","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Feltöltés","","","kg","","0.76"]
["","Típus","","","","","R-32"]
["Működési tartomány","Hűtés","Környezeti","Max.","°C száraz hőm.","","50 (4), 46 (5)"]
["","","","Min.","°C száraz hőm.","","-10"]
["Csőcsatlakozások","Szintkülönbség","IU - OU","Max.","m","","15"]
["","További hűtőközeg utántöltés","","","kg/m","","0,02 (10m-t meghaladó csőhosszhoz)"]
["Kompresszor","Típus","","","","","Hermetikusan zárt lengő kompresszor"]
["Méretek","Egység","","Szélesség","mm","","840"]
["","","","Mélység","mm","","350"]
["","","","Magasság","mm","","552"]
["Tömeg","Egység","","","kg","","32"]
["Power supply","fázis","","","","","1~"]
["","Frekvencia","","","Hz","","50"]
["","Feszültség","","","V","","220-240"]
["Notes","","","","","(1) - Csak az alábbiakkal együtt lehetséges: ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["","","","","","(2) - Csak az alábbiakkal együtt lehetséges: ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","","(3) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","","(4) - Csak az alábbiakkal együtt lehetséges: ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Csak az alábbiakkal együtt lehetséges: ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Méretek","Egység","","Magasság","mm","552"]
["","","","Szélesség","mm","840"]
["","","","Mélység","mm","350"]
["Tömeg","Egység","","","kg","32"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10"]
["","","","Max.","°C száraz hőm.","50 (4), 46 (5)"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","46.0"]
["","Fűtés","","Névl.","dB(A)","47.0"]
["Hűtőközeg","Töltet","","","kg","0.76"]
["","Töltet","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Áramellátás","Frekvencia","","","Hz","50"]