{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Hangnyomás szint","Fűtés","","Magas","dBA","","","47","48"]
["","","","Névl.","dBA","","52","","","49"]
["","Hűtés","","Magas","dBA","","","46","48"]
["","","","Névl.","dBA","","52","","","49"]
["Standard Accessories","Leeresztő csavar","","","","","1","1","1","1"]
["","Telepítési utasítás","","","","","1","1","1","1"]
["","Hűtőközeg töltési címke","","","","","1","1","","1"]
["","Fluorinált káros gázokra vonatkozó többnyelvű címke","","","","","1","1","","1"]
["Refrigerant","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Feltöltés","","","kg","","1.70","1.0","1.2","1.50"]
["","Type","","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilátormotor","Sebesség","Hűtés","Szuper alacsony","ford./perc","","","780","780"]
["","","Fűtés","Szuper alacsony","ford./perc","","","740","740"]
["Üzemi tartomány","Hűtés","Környezeti","Max.","°C száraz hőm.","","46","46","46","46"]
["","","","Min.","°C száraz hőm.","","-10","10","10","-10"]
["","Fűtés","Környezeti","Max.","°C párás hőm.","","18","18","18","18"]
["","","","Min.","°C párás hőm.","","-15","-15","-15","-15"]
["Piping connections","Szintkülönbség","IU - OU","Max.","m","","20.0","15","15","20.0"]
["","További hűtőközeg utántöltés","","","kg/m","","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["Hangteljesítmény szintje","Hűtés","","","dBA","","65","","","62"]
["","Fűtés","","","dBA","","65","","","62"]
["Kompresszor","Típus","","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Méretek","Egység","","Szélesség","mm","","825","765","765","825"]
["","","","Mélység","mm","","300","285","285","300"]
["","","","Magasság","mm","","735","550","550","735"]
["Tömeg","Egység","","","kg","","47","34","34","47"]
["Fan","Légszállítási sebesség","Fűtés","Szuper alacsony","cfm","","","904","904"]
["","","","Szuper alacsony","m³/perc","","","25.6","25.6"]
["","","Cooling","Szuper alacsony","m³/perc","","","30.1","30.1"]
["","","","Szuper alacsony","cfm","","","1,063","1,063"]
["Power supply","Phase","","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","","50","50","50","50"]
["","Feszültség","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Notes","","","","","(1) - 220V","","(1) - Multi rendszerű kültéri egységhez való csatlakoztatás esetén lásd a csatlakoztatandó multi kültéri egység műszaki jellemzőit","(1) - Multi rendszerű kültéri egységhez való csatlakoztatás esetén lásd a csatlakoztatandó multi kültéri egység műszaki jellemzőit"]
["","","","","","(2) - 230V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230V","(3) - 230V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(5) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","48.9"]
["","","Fűtés","Szuper alacsony","m³/perc","43.1"]
["","","","Szuper alacsony","cfm","1727"]
["","","Fűtés","Szuper alacsony","cfm","1522"]
["Méretek","Egység","","Magasság","mm","735"]
["","","","Szélesség","mm","825"]
["","","","Mélység","mm","300"]
["Tömeg","Egység","","","kg","47"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","ford./perc","670"]
["","","Fűtés","Szuper alacsony","ford./perc","670"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","10"]
["","","","Max.","°C száraz hőm.","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15"]
["","","","Max.","°C párás hőm.","18"]
["Hangnyomás szint","Hűtés","","Magas","dBA","48"]
["","Fűtés","","Magas","dBA","48"]
["Hűtőközeg","Típus","","","","R-410A"]
["","Töltet","","","kg","1.7"]
["","Töltet","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","30"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","20"]
["Standard Accessories","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]
["Notes","","","","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]