{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","","48"]
["","","","Alacsony","dB(A)","","45"]
["Standard Accessories","1","","","","","550"]
["Hűtőközeg","Feltöltés","","","kg","","2.5"]
["","Típus","","","","","1.2"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","","30.1"]
["","","","Szuper alacsony","cfm","","1,063"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","","740"]
["","","Fűtés","Szuper alacsony","1/perc","","-15"]
["Üzemi tartomány","Fűtés","Környezeti","Min.","°C párás hőm.","","20"]
["","","","Max.","°C párás hőm.","","10"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","44"]
["","","","Magas","dB(A)","","48"]
["Kompresszor","Típus","","","","","Hermetikusan zárt lengő kompresszor"]
["Méretek","Egység","","Szélesség","mm","","285"]
["","","","Mélység","mm","","612"]
["","","","Magasság","mm","","765"]
["Tömeg","Egység","","","kg","","34"]
["Ventilátor","Légáramlási arány","Fűtés","Szuper alacsony","cfm","","904"]
["","","","Szuper alacsony","m³/perc","","25.6"]
["Power supply","fázis","","","","","1~"]
["","Frekvencia","","","Hz","","50"]
["","Feszültség","","","V","","220-240"]
["Notes","","","","","(1) - 220V","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["","","","","","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230V"]
["","","","","","","(4) - 240V"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","30.1"]
["","","Fűtés","Szuper alacsony","m³/perc","25.6"]
["","","","Szuper alacsony","cfm","1063"]
["","","Fűtés","Szuper alacsony","cfm","904"]
["Méretek","Egység","","Magasság","mm","550"]
["","","","Szélesség","mm","765"]
["","","","Mélység","mm","285"]
["Tömeg","Egység","","","kg","34"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","780"]
["","","Fűtés","Szuper alacsony","1/perc","740"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","10"]
["","","","Max.","°C száraz hőm.","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15"]
["","","","Max.","°C párás hőm.","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","46"]
["","Fűtés","","Magas","dB(A)","47"]
["","","","Alacsony","dB(A)","44"]
["Hűtőközeg","Típus","","","","R-410A"]
["","Töltet","","","kg","1.0"]
["","Töltet","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]