{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Hangnyomás szint","Fűtés","","Magas","dBA","40","42","44","45"]
["","","","Közepes","dBA","34","38","40","41"]
["","","","Csendes működés","dBA","21","30","32","33"]
["","","","Alacsony","dBA","28","33","35","36"]
["","Hűtés","","Közepes","dBA","33","39","41","42"]
["","","","Csendes működés","dBA","20","31","33","34"]
["","","","Alacsony","dBA","26","34","36","37"]
["","","","Magas","dBA","40","43","45","46"]
["Standard Accessories","Telepítési utasítás","","","","1","1","1","1"]
["","Használati utasítás","","","","1","1","1","1"]
["","Infravörös távirányító","","","","1","1","1","1"]
["","AAA szárazelemek","","","","2","2","2","2"]
["","Távirányító tartó","","","","1","1","1","1"]
["","Szerelőlemez","","","","1","1","1","1"]
["","Beltéri egység rögzítő csavarja","","","","2","2","2","2"]
["Vezérlőrendszerek","Wired remote control","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.50","12.7","12.7","12.7"]
["","Ürítés","","","","18","18","18","18"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.019","0.029","0.032","0.032"]
["","Fűtés","","Névl.","kW","0.020","0.032","0.035","0.035"]
["Sound power level","Hűtés","","","dBA","55","59","60","62"]
["","Fűtés","","","dBA","55","61","62","62"]
["Méretek","Egység","","Szélesség","pp","770","990","990","990"]
["","","","Mélység","pp","225","263","263","263"]
["","","","Magasság","pp","286","295","295","295"]
["Casing","Colour","","","","Fehér","Fehér","Fehér","Fehér"]
["Tömeg","Egység","","","kg","8.50","13.5","13.5","13.5"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","10.3","17.3","17.9","17.9"]
["","","","Alacsony","m³/perc","6.7","12.2","12.8","12.8"]
["","","","Medium","m³/perc","8.6","14.8","15.8","15.8"]
["","","","Csendes működés","m³/perc","5.3","10.7","11.3","11.3"]
["","","Hűtés","Alacsony","m³/perc","6.1","11.9","12.2","12.2"]
["","","","Medium","m³/perc","8.1","14.4","14.8","14.8"]
["","","","Magas","m³/perc","10.1","16.8","17.3","17.3"]
["","","","Csendes működés","m³/perc","4.4","10.5","10.7","10.7"]
["Áramellátás","Phase","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Megnevezés","","","","","V1","V1","V1"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","","","","0.019","0.032"]
["","Fűtés","","Névl.","kW","","","","","0.02","0.032"]
["Burkolat","Szín","","","","","","","","Fehér","Fehér"]
["Méretek","Egység","","Magasság","pp","","","","","286","286"]
["","","","Szélesség","pp","","","","","770","770"]
["","","","Mélység","pp","","","","","225","225"]
["Tömeg","Egység","","","kg","","","","","8.5","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","","","","10.1","11.5"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","","","","8.1","8.3"]
["","","","Alacsony","m³/perc","","","","","6.1","6.3"]
["","","","Csendes működés","m³/perc","","","","","4.4","4.5"]
["","","Fűtés","Magas","m³/perc","","","","","10.3","11.5"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","","","","8.6","9"]
["","","Fűtés","Alacsony","m³/perc","","","","","6.7","7"]
["","","","Csendes működés","m³/perc","","","","","5.3","5.3"]
["Hangteljesítményszint","Hűtés","","","dBA","","","","","55","58"]
["","Fűtés","","","dBA","","","","","55","58"]
["Hangnyomás szint","Hűtés","","Magas","dBA","","","","","40","43"]
["Hangnyomásszint","Hűtés","","Közepes","dBA","","","","","33","34"]
["Hangnyomás szint","Hűtés","","Alacsony","dBA","","","","","26","27"]
["","","","Csendes működés","dBA","","","","","20","20"]
["","Fűtés","","Magas","dBA","","","","","40","40"]
["Hangnyomásszint","Fűtés","","Közepes","dBA","","","","","34","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dBA","","","","","28","29"]
["","","","Csendes működés","dBA","","","","","21","21"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","","","","","6.35","6.35"]
["","Gáz","","Külső átm.","pp","","","","","9.5","9.5"]
["","Ürítés","","","","","","","","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","","","","ARC470A1","ARC470A1"]
["","Vezetékes távszabályzó","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Áramellátás","fázis","","","","","","","","1~","1~"]
["","Frekvencia","","","Hz","","","","","50","50"]
["","Feszültség","","","V","","","","","220-240","220-240"]