{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-G"]
[]
[]
[]
[]
["","","","","","ATXF25G5V1B","ATXF35G5V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.023","0.029"]
["","Fűtés","","Névl.","kW","0.023","0.023"]
["Burkolat","Szín","","","","Fehér","Fehér"]
["Méretek","Egység","","Magasság","mm","286","286"]
["","","","Szélesség","mm","770","770"]
["","","","Mélység","mm","225","225"]
["Tömeg","Egység","","","kg","8.5","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","9.8","10.9"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8","7"]
["","","","Alacsony","m³/perc","6","5.7"]
["","","","Csendes működés","m³/perc","4.3","4.6"]
["","","Fűtés","Magas","m³/perc","10.4","9.3"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.4","7.5"]
["","","Fűtés","Alacsony","m³/perc","6.4","6"]
["","","","Csendes működés","m³/perc","5.3","5.2"]
["Hangteljesítményszint","Hűtés","","","dB(A)","54","54"]
["","Fűtés","","","dB(A)","55","56"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","40","56"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","26"]
["","","","Csendes működés","dB(A)","20"]
["","Fűtés","","Magas","dB(A)","40","40"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","28","29"]
["","","","Csendes működés","dB(A)","21","21"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6","6"]
["","Gáz","","Külső átm.","mm","9.5","9.5"]
["","Ürítés","","","","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC480A93","ARC480A93"]
["","Vezetékes távszabályzó","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-440","220-440"]
["Notes","","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 5 m; szintkülönbség: 0m","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 5 m; szintkülönbség: 0m"]
["","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m (vízszintes)","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m (vízszintes)"]
["","","","","","(3) - Az elektromos adatokat lásd külön rajzokon","(3) - Az elektromos adatokat lásd külön rajzokon"]