{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Hűtési teljesítmény","Min.","","kW","","","1.40"]
["","Max.","","kW","","","4.00"]
["","Névl.","","kW","","","3.40"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","","402"]
["","EER","","","","","4.23"]
["","COP","","","","","4.04"]
["","Energiacímkézés irányelve","Hűtés","","","","A"]
["","","Fűtés","","","","A"]
["Fűtőkapacitás","Névl.","","kW","","","4.00"]
["","Min.","","kW","","","1.40"]
["","Max.","","kW","","","5.20"]
["Notes","","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","","(2) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","","(3) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","","(4) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["Hűtési teljesítmény","Min.","","kW","1.30","1.30","","1.40"]
["","Névl.","","kW","2.50","2.50","","3.40"]
["","Max.","","kW","3.20","3.20","","4.00"]
["Fűtőkapacitás","Min.","","kW","1.30","1.30","","1.40"]
["","Névl.","","kW","2.80","2.80","","4.00"]
["","Max.","","kW","4.70","4.70","","5.20"]
["Névleges hatékonyság","EER","","","4.50","4.50","","4.23"]
["","COP","","","5.00","5.00","","4.04"]
["","Éves energiafogyasztás","","kWh","278","278","","402"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A","A","","A"]
["","","Fűtés","","A","A","","A"]
["Felülethűtés","Energiatakarékossági osztály","","","A+++","A+++","","A+++"]
["","Kapacitás","Pdesign","kW","2.50","2.50","","3.40"]
["","SEER","","","8.55","8.55","","8.55"]
["","Éves energiafogyasztás","","kWh/a","102","102","","139"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A+++","A+++","","A+++"]
["","Kapacitás","Pdesign","kW","2.40","2.40","","2.50"]
["","SCOP/A","","","5.10","5.10","","5.10"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","2.30","2.30","","2.35"]
["","Éves energiafogyasztás","","kWh/a","659","659","","686"]
["Energiatakarékossági besorolás","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]