{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-L"]
[]
[]
[]
[]
["","","","","","ATXP20L2V1B","ATXP20L5V1B","ATXP25L2V1B","ATXP25L5V1B","ATXP35L2V1B","ATXP35L5V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.017","0.017","0.019","0.019","0.032","0.032"]
["","Fűtés","","Névl.","kW","0.02","0.02","0.02","0.02","0.032","0.032"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér","Fehér","Fehér","Fehér"]
["Méretek","Egység","","Magasság","pp","286","286","286","286","286","286"]
["","","","Szélesség","pp","770","770","770","770","770","770"]
["","","","Mélység","pp","225","225","225","225","225","225"]
["Tömeg","Egység","","","kg","9","9","9","9","9","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","9.8","9.8","10.1","10.1","11.5","11.5"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","7.9","7.9","8.1","8.1","8.3","8.3"]
["","","","Alacsony","m³/perc","5.9","5.9","6.1","6.1","6.3","6.3"]
["","","","Csendes működés","m³/perc","4.4","4.4","4.4","4.4","4.5","4.5"]
["","","Fűtés","Magas","m³/perc","10.3","10.3","10.3","10.3","11.5","11.5"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.4","8.4","8.6","8.6","9","9"]
["","","Fűtés","Alacsony","m³/perc","6.5","6.5","6.7","6.7","7","7"]
["","","","Csendes működés","m³/perc","5.3","5.3","5.3","5.3","5.3","5.3"]
["Hangteljesítményszint","Hűtés","","","dB(A)","55","55","55","55","58","58"]
["","Fűtés","","","dB(A)","55","55","55","55","58","58"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39","39","40","40","43","43"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","33","33","33","34","34"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","25","26","26","27","27"]
["","","","Csendes működés","dB(A)","20","20","20","20","20","20"]
["","Fűtés","","Magas","dB(A)","39","39","40","40","40","40"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34","34","34","34","35","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","28","28","28","28","29","29"]
["","","","Csendes működés","dB(A)","21","21","21","21","21","21"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.5","9.5","9.5","9.5","9.5","9.5"]
["","Ürítés","","","","18","18","18","18","18","18"]
["Control systems","Infrared remote control","","","","","","ARC480A11","ARC480A11"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC480A11","ARC480A11","","","ARC480A11","ARC480A11"]