{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B","ATXP25N5V1B","ATXP35N5V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.019","0.02","0.032"]
["","Fűtés","","Névl.","kW","0.023","0.023","0.032"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér"]
["Méretek","Egység","","Magasság","mm","286","286","286"]
["","","","Szélesség","mm","770","770","770"]
["","","","Mélység","mm","225","225","225"]
["Tömeg","Egység","","","kg","8.5","8.5","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","9.5","9.7","11.5"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","7.4","7.7","8.3"]
["","","","Alacsony","m³/perc","5.6","5.8","6.3"]
["","","","Csendes működés","m³/perc","4.2","4.2","4.5"]
["","","Fűtés","Magas","m³/perc","10.4","10.4","11.5"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.1","8.1","9"]
["","","Fűtés","Alacsony","m³/perc","6.2","6.4","7"]
["","","","Csendes működés","m³/perc","5.2","5.2","5.3"]
["Hangteljesítményszint","Hűtés","","","dB(A)","55","55","58"]
["","Fűtés","","","dB(A)","55","55","58"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39","40","43"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","33","34"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","26","27"]
["","","","Csendes működés","dB(A)","19","19","20"]
["","Fűtés","","Magas","dB(A)","39","40","40"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34","34","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","28","28","29"]
["","","","Csendes működés","dB(A)","21","21","21"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6","6","6"]
["","Gáz","","Külső átm.","mm","9.5","9.5","9.5"]
["","Ürítés","","","","18","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Vezetékes távszabályzó","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1"]
["","Silver particle filter","","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]