{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTP-K"]
[]
[]
[]
[]
["","","","","","ATXTP25K3V1B","ATXTP35K3V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.03","0.03"]
["","Fűtés","","Névl.","kW","0.035","0.035"]
["Burkolat","Szín","","","","Fehér","Fehér"]
["Méretek","Egység","","Magasság","pp","285","285"]
["","","","Szélesség","pp","770","770"]
["","","","Mélység","pp","225","225"]
["Tömeg","Egység","","","kg","9","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","10.6","11.4"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","7.7","8.2"]
["","","","Alacsony","m³/perc","5.3","5.4"]
["","","","Csendes működés","m³/perc","4.3","4.3"]
["","","Fűtés","Magas","m³/perc","11.2","10.8"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8","7.8"]
["","","Fűtés","Alacsony","m³/perc","5.8","5.8"]
["","","","Csendes működés","m³/perc","4.9","4.9"]
["Hangteljesítményszint","Hűtés","","","dB(A)","58","58"]
["","Fűtés","","","dB(A)","58","58"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","43","43"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","35","35"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","26","26"]
["","","","Csendes működés","dB(A)","21","21"]
["","Fűtés","","Magas","dB(A)","43","43"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","35","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","26","26"]
["","","","Csendes működés","dB(A)","21","21"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.5","9.5"]
["","Ürítés","","","","16 (a csatlakozótömlő belső átmérője)","16 (a csatlakozótömlő belső átmérője)"]
["Control systems","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Áramellátás","Megnevezés","","","","V1","V1"]
["","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]