{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Hűtési teljesítmény","Hűtési összteljesítmény","","Névl.","kW","12.10"]
["Fűtési teljesítmény","Összes teljesítmény","","Névl.","kW","13.5"]
["Burkolat","Szín","","","","Friss fehér"]
["Méretek","Egység","","Magasság","pp","1850"]
["","","","Szélesség","pp","600"]
["","","","Mélység","pp","350"]
["Tömeg","Egység","","","kg","50"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","28"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","26"]
["","","","Alacsony","m³/perc","24"]
["","","Fűtés","Magas","m³/perc","28"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","26"]
["","","Fűtés","Alacsony","m³/perc","24"]
["Hangteljesítményszint","Hűtés","","","dB(A)","63"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","51"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","48"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","46"]
["","Fűtés","","Magas","dB(A)","51"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","46"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","48"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","9.52"]
["","Gáz","","Külső átm.","pp","15.9"]
["","Ürítés","","","","I.D. 20/O.D. 26"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50/60"]
["","Feszültség","","","V","220-240/220"]