{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000676"]
[]
[]
[]
[]
["","","","","","BR00000676."]
["Személyre szabható","","","","","Padlón álló típus"]
["Teljesítmény","m³/perc","","","","33.33"]
["Burkolat","Szín","","","","Festett galvanizált acélbevonat"]
["Méretek","Egység","","Magasság","mm","1628"]
["","","","Szélesség","mm","720"]
["","","","Mélység","mm","770"]
["Tömeg","Egység","","","kg","150"]
["Személyre szabható szobaterület","m²","","","","133"]
["Légtisztító működés","Elektromos bemenet","","H","kW","0.379"]
["Hangnyomás szint","Légtisztító működés","","Magas","dB(A)","55.9"]
["Ventilátor","Légáramlási arány","Légtisztító működés","Turbó","m³/óra","2300"]
["","","","Magas","m³/óra","2000"]
["Biztonsági berendezések","Tétel","","01","","Biztonsági kapcsoló (a hátsó ajtó kinyílása esetén a működés leáll)"]
["Standard Accessories","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Hálózati csatlakozózsinór","m","","","","3"]
["Áramellátás","Frekvencia","","","Hz","50/60"]
["Működési áram","Légtisztító működés","","Magas","A","1.73"]