{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-N7"]
[]
[]
[]
[]
["","","","","","CHYHBH05AFV32 / 3MXM52N2V1B7"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","A"]
["COP","","","","","4.49 (1)"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","Seasonal space heating eff. class","","A+"]
["","","","ηs (Szezonális felületfűtési hatékonyság)","%","111.4"]
["","","","SCOP","","2.86"]
["Fűtőkapacitás","Névl.","","","kW","4.41 (1)"]
["Notes","","","","","(1) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 35 °C (Hőm. különbség = 5 °C), kazán kihagyva"]