{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CKHWS-BV3"]
[]
[]
[]
[]
["","","","","","CKHWS180BJV3","CKHWS230BJV3"]
["Befoglaló méretek","Berendezés","Magasság","Tartály","mm","1655","1855"]
["Méretek","Egység","","Szélesség","mm","595","595"]
["","","","Mélység","mm","634","634"]
["Súly","Berendezés","","Üres","kg","106","115"]
["Tartály","Vízmennyiség","","","l","180","230"]
["","Anyag","","","","Rozsdamentes acél (1.4521)","Rozsdamentes acél (1.4521)"]
["","Maximális vízhőmérséklet","","","°C","65.0","65.0"]
["","Energiahatékonysági osztály","","","","B","B"]
["Tartalék fűtőelem","Teljesítmény","","","kW","1.5","1.5"]
["Notes","","","","","(1) - 45 K dT-je alapján","(1) - 45 K dT-je alapján"]
["","","","","","(2) - DHW áramlás","(2) - DHW áramlás"]
["","","","","","(3) - 2 pólusú 10A, görbe 230V","(3) - 2 pólusú 10A, görbe 230V"]
["","","","","","(4) - A hidraulikus doboz fent említett áramellátása csak a tartalékfűtőhöz való. A hidraulikus doboz kapcsolódobozát és szivattyúját a kültéri egységgel szállítjuk.","(4) - A hidraulikus doboz fent említett áramellátása csak a tartalékfűtőhöz való. A hidraulikus doboz kapcsolódobozát és szivattyúját a kültéri egységgel szállítjuk."]