{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","39"]
["","","Közepes","dB(A)","32"]
["","","Csendes működés","dB(A)","21"]
["","","Alacsony","dB(A)","25"]
["","Hűtés","Közepes","dB(A)","32"]
["","","Csendes működés","dB(A)","21"]
["","","Alacsony","dB(A)","25"]
["","","Magas","dB(A)","39"]
["Standard Accessories","Telepítési utasítás","","","1"]
["","Használati utasítás","","","1"]
["","Légszűrő","","","2"]
["","Infravörös távirányító","","","1"]
["","A távirányító rögzítésére szolgáló lap","","","1"]
["","Csavarzsák","","","1"]
["","Csavarfedél","","","1"]
["","AAA szárazelemek","","","2"]
["","Általános biztonsági óvintézkedések","","","1"]
["Hűtőközeg","GWP","","","675.0"]
["Vezérlőrendszerek","Wired remote control","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","6.35"]
["","Gáz","Külső átm.","mm","9.50"]
["","Ürítés","","","18"]
["Áramfelvétel","Hűtés","Névl.","kW","0.020"]
["","Fűtés","Névl.","kW","0.020"]
["Sound power level","Hűtés","","dB(A)","57"]
["Méretek","Egység","Szélesség","mm","798"]
["","","Mélység","mm","189"]
["","","Magasság","mm","295"]
["Burkolat","Szín","","","Fekete fa"]
["Tömeg","Egység","","kg","12"]
["Power supply","fázis","","","1~"]
["","Frekvencia","","Hz","50"]
["","Megnevezés","","","V1"]
["","Feszültség","","V","220-240"]