{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AW"]
[]
[]
[]
[]
["","","","","","CTXA15A2V1BW"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","39"]
["","","","Közepes","dB(A)","32"]
["","","","Csendes működés","dB(A)","21"]
["","","","Alacsony","dB(A)","25"]
["","Hűtés","","Medium","dB(A)","32"]
["","","","Csendes működés","dB(A)","21"]
["","","","Alacsony","dB(A)","25"]
["","","","Magas","dB(A)","39"]
["Standard Accessories","Telepítési utasítás","","","","1"]
["","Használati utasítás","","","","1"]
["","Légszűrő","","","","2"]
["","Infravörös távirányító","","","","1"]
["","A távirányító rögzítésére szolgáló lap","","","","1"]
["","Csavarzsák","","","","1"]
["","Csavarfedél","","","","1"]
["","AAA szárazelemek","","","","2"]
["","Általános biztonsági óvintézkedések","","","","1"]
["Refrigerant","GWP","","","","675.0"]
["Control systems","Wired remote control","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35"]
["","Gáz","","Külső átm.","mm","9.50"]
["","Ürítés","","","","18"]
["Teljesítményfelvétel","Hűtés","","Névl.","kW","0.020"]
["","Fűtés","","Névl.","kW","0.020"]
["Sound power level","Hűtés","","","dB(A)","57"]
["Méretek","Egység","","Szélesség","mm","798"]
["","","","Mélység","mm","189"]
["","","","Magasság","mm","295"]
["Burkolat","Szín","","","","Fehér"]
["Tömeg","Egység","","","kg","12"]
["Ventilátor","Légszállítási sebesség","Fűtés","Magas","m³/perc","10.9"]
["","","","Medium","m³/perc","8.7"]
["","","","Alacsony","m³/perc","6.4"]
["","","","Csendes működés","m³/perc","4.5"]
["","","Hűtés","Alacsony","m³/perc","6.1"]
["","","","Medium","m³/perc","8"]
["","","","Magas","m³/perc","11.0"]
["","","","Csendes működés","m³/perc","4.6"]
["Áramellátás","fázis","","","","1~"]
["","Megnevezés","","","","V1"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]