{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Power input","Hűtés","","Névl.","kW","0.020"]
["","Fűtés","","Névl.","kW","0.020"]
["Burkolat","Szín","","","","Fekete"]
["Méretek","Egység","","Magasság","pp","295"]
["","","","Szélesség","pp","798"]
["","","","Mélység","pp","189"]
["Súly","Egység","","","kg","11.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","11.0"]
["","","","Közepes","m³/perc","8.2"]
["","","","Alacsony","m³/perc","6.1"]
["","","","Csendes működés","m³/perc","4.6"]
["","","Fűtés","Magas","m³/perc","10.9"]
["","","","Közepes","m³/perc","8.7"]
["","","","Alacsony","m³/perc","6.4"]
["","","","Csendes működés","m³/perc","4.5"]
["Hangteljesítményszint","Hűtés","","","dB(A)","57"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39"]
["","","","Közepes","dB(A)","32"]
["","","","Alacsony","dB(A)","25"]
["","","","Csendes működés","dB(A)","21"]
["","Fűtés","","Magas","dB(A)","39"]
["","","","Közepes","dB(A)","32"]
["","","","Alacsony","dB(A)","25"]
["","","","Csendes működés","dB(A)","21"]
["Refrigerant","GWP","","","","675.0"]
["Piping connections","Folyadék","","Külső átm.","pp","6.35"]
["","Gáz","","Külső átm.","pp","9.50"]
["","Ürítés","","","","18"]
["Vezérlőrendszerek","Infrared remote control","","","","ARC466A85"]
["","Wired remote control","","","","BRC073A1"]
["Standard Accessories","Telepítési utasítás","","","","1"]
["","Használati utasítás","","","","1"]
["","Légszűrő","","","","2"]
["","Infravörös távirányító","","","","1"]
["","A távirányító rögzítésére szolgáló lap","","","","1"]
["","Csavarzsák","","","","1"]
["","Csavarfedél","","","","2"]
["","AAA szárazelemek","","","","2"]
["","Általános biztonsági óvintézkedések","","","","1"]
["Power supply","Megnevezés","","","","V1"]
["","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]