{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CS"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BS"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.02"]
["","Fűtés","","Névl.","kW","0.02"]
["Burkolat","Szín","","","","Ezüst"]
["Méretek","Egység","","Magasság","pp","295"]
["","","","Szélesség","pp","798"]
["","","","Mélység","pp","189"]
["Tömeg","Egység","","","kg","11.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","11"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8.2"]
["","","","Alacsony","m³/perc","6.1"]
["","","","Csendes működés","m³/perc","4.6"]
["","","Fűtés","Magas","m³/perc","10.9"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.7"]
["","","Fűtés","Alacsony","m³/perc","6.4"]
["","","","Csendes működés","m³/perc","4.5"]
["Hangteljesítményszint","Hűtés","","","dB(A)","57"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","32"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25"]
["","","","Csendes működés","dB(A)","21"]
["","Fűtés","","Magas","dB(A)","39"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","32"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","25"]
["","","","Csendes működés","dB(A)","21"]
["Hűtőközeg","GWP","","","","675"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35"]
["","Gáz","","Külső átm.","pp","9.5"]
["","Ürítés","","","","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A85"]
["","Vezetékes távszabályzó","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Légszűrő","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["Áramellátás","Megnevezés","","","","V1"]
["","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]