{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","38","","41"]
["","","","Csendes működés","dB(A)","21","","21"]
["","","","Alacsony","dB(A)","28","","30"]
["","Hűtés","","Csendes működés","dB(A)","21","","21"]
["","","","Alacsony","dB(A)","25","","28"]
["","","","Magas","dB(A)","37","","42"]
["","","","Névl.","dB(A)","33"]
["","Hűtés","","Névl.","dB(A)","31","","35"]
["Standard Accessories","Telepítési utasítás","","","","1","","1"]
["","Használati utasítás","","","","1","","1"]
["","Vezeték nélküli távirányító","","","","1","","1"]
["","Elemek","","","","2","","2"]
["","Távirányító tartó","","","","1","","1"]
["","Szerelőlemez","","","","1","","1"]
["","Beltéri egység rögzítő csavarja","","","","2","","2"]
["","Titánium apatit fotokatalitikus légtisztító szűrő","","","","2","","2"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A6","","ARC466A6"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","","6.35"]
["","Gáz","","Külső átm.","mm","9.5","","9.5"]
["","Drain","","","","18","","18"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.040","","0.040"]
["","Fűtés","","Névl.","kW","0.040","","0.040"]
["Sound power level","Hűtés","","","dB(A)","55","","59"]
["","Fűtés","","","dB(A)","56","","58"]
["Méretek","Egység","","Szélesség","mm","780","","780"]
["","","","Mélység","mm","215","","215"]
["","","","Magasság","mm","289","","289"]
["Burkolat","Szín","","","","Fehér","","Fehér"]
["Tömeg","Egység","","","kg","8","","8"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","","","10.1"]
["","","","Alacsony","m³/perc","","","6.3"]
["","","","Csendes működés","m³/perc","","","4.3"]
["","","Hűtés","Alacsony","m³/perc","","","5.2"]
["","","","Magas","m³/perc","","","9.2"]
["","","","Csendes működés","m³/perc","","","3.9"]
["","","","Névl.","m³/perc","","","8.1"]
["","","Hűtés","Névl.","m³/perc","","","7.2"]
["Power supply","fázis","","","","1~","","1~"]
["","Frekvencia","","","Hz","50","","50"]
["","Megnevezés","","","","V1","","V1"]
["","Feszültség","","","V","220-240","","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","0.04","","0.040"]
["","Fűtés","","Névl.","kW","","0.04","","0.040"]
["Burkolat","Szín","","","","","Fehér","","Fehér"]
["Méretek","Egység","","Magasság","mm","","289","","289"]
["","","","Szélesség","mm","","780","","780"]
["","","","Mélység","mm","","215","","215"]
["Tömeg","Egység","","","kg","","8","","8.00"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","7.9","","9.2"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","6.3","","7.2"]
["","","","Alacsony","m³/perc","","4.7","","5.2"]
["","","","Csendes működés","m³/perc","","3.9","","3.9"]
["","","Fűtés","Magas","m³/perc","","9","","10.1"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","7.5","","8.1"]
["","","Fűtés","Alacsony","m³/perc","","6","","6.3"]
["","","","Csendes működés","m³/perc","","4.3","","4.3"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","55","","59"]
["","Fűtés","","","dB(A)","","56","","58"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","37","","42"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","31","","35"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","25","","28"]
["","","","Csendes működés","dB(A)","","21","","21"]
["","Fűtés","","Magas","dB(A)","","38","","41"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","33","","36"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","","28","","30"]
["","","","Csendes működés","dB(A)","","21","","21"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","6.35","","6.35"]
["","Gáz","","Külső átm.","mm","","9.5","","9.50"]
["","Ürítés","","","","","18","","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","ARC466A6","","ARC466A6"]
["Standard Accessories","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Áramellátás","Megnevezés","","","","","V1","","V1"]
["","fázis","","","","","1~","","1~"]
["","Frekvencia","","","Hz","","50","","50"]
["","Feszültség","","","V","","220-240","","220-240"]