{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Áramfelvétel","kW","","","","0.015"]
["A csatlakoztatható beltéri egységek maximális száma:","","","","","32"]
["A csatlakoztatható kültéri egységek maximális száma: @","","","","","7"]
["Méretek","Egység","","Magasság","mm","136"]
["","","","Szélesség","mm","384"]
["","","","Mélység","mm","92"]
["Kommunikáció","DIII-NET","","Mennyiség","","1"]
["","","","Megjegyzés","","DIII-NET (F1F2)"]
["","Ethernet","","Mennyiség","","1"]
["","Bemeneti terminál","Digitális","Mennyiség","","4"]
["Külső hőmérséklet","Működés","","Min.","°C","-10"]
["","","","Max.","°C","50"]
["","Tárolás","","Min.","°C","-20"]
["","","","Max.","°C","60"]
["","Külső hőmérséklet-=-Relatív páratartalom <-=-%","","","%","85"]
["Áramellátás","Frekvencia","","","Hz","50/60"]
["","Feszültség","","","V","110-240 AC"]
["Notes","","","","","(1) - Tartalmazza a WAGO tápegység felvett teljesítményét, a CPU modult és a I/O modult"]
["","","","","","(2) - A méretek tartalmazzák a WAGO tápegységet, a CPU modulokat, a I/O modult és a szükséges helyet a különböző részek között"]
["","","","","","(3) - A választható képernyő méretei a következők: magasság: 209mm, szélesség: 123mm, mélység: 8,5mm"]