{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":11,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVX-D9WG / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","","EAVX16S18DA9WG / EPGA11DAV3","EAVX16S23DA9WG / EPGA11DAV3","EAVX16S18DA9WG / EPGA14DAV3","EAVX16S23DA9WG / EPGA14DAV3","EAVX16S18DA9WG / EPGA16DAV3","EAVX16S23DA9WG / EPGA16DAV3"]
["Használati melegvíz fűtés","Általános","","Terhelési profil","","","","L","XL","L","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","","","A","A","A","A"]
["COP","","","","","5.15, 3.88","5.15, 3.88","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Indoor unit","","","","","EAVX16S18DA9W","EAVX16S23DA9W","EAVX16S18DA9W","EAVX16S23DA9W","EAVX16S18DA9W","EAVX16S23DA9W"]
["Hűtési teljesítmény","Névl.","","","kW","","","11.1 (1), 11.9 (2)","11.1 (1), 11.9 (2)","13.5 (1), 11.9 (2)","13.5 (1), 11.9 (2)"]
["EER","","","","","4.75, 3.23","4.75, 3.23","4.09 (1), 2.99 (2)","4.09 (1), 2.99 (2)","3.94 (1), 2.99 (2)","3.94 (1), 2.99 (2)"]
["Fűtőkapacitás","Névl.","","","kW","","","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","","2.72 (1), 3.97 (2)","2.72 (1), 3.97 (2)","3.42 (1), 3.97 (2)","3.42 (1), 3.97 (2)"]
["","Fűtés","","Névl.","kW","","","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["Notes","","","","","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["Fűtőkapacitás","Névl.","","","kW","11.1, 11.3","11.1, 11.3"]
["Hűtési teljesítmény","Névl.","","","kW","10.5, 10.7","10.5, 10.7"]
["Elektromos bemenet","Fűtés","","Névl.","kW","2.16, 2.91","2.16, 2.91"]
["","Hűtés","","Névl.","kW","2.21, 3.30","2.21, 3.30"]
["Áramfelvétel","Háztartási melegvíz 10°C és 50°C között","","Névl.","kWh","2.67","3.08"]
["Felmelegedési idő 10°C-ról 50°C-ra","ó","","","","9 óra 20 perc 7°C környezeti hőmérsékleten","9 óra 20 perc 7°C környezeti hőmérsékleten"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","L","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","A","A"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","3.32","3.32"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A++","A++"]
["","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","4.44","4.44"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++","A+++"]