{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLA09-14D3V3"]
[]
[]
[]
[]
["","","","","","EBLA09DA3V3","EBLA11DA3V3","EBLA14DA3V3"]
["Fűtőkapacitás","Névl.","","","kW","9.37 (1), 9.00 (2)","10.6 (1), 9.82 (2)","12.0 (1), 12.5 (2)"]
["Hűtési teljesítmény","Névl.","","","kW","9.35 (3), 9.10 (4)","11.6 (3), 11.5 (4)","12.8 (3), 12.7 (4)"]
["Fűtőtest kapacitása","1 lépés","","","kW","3","3","3"]
["Elektromos bemenet","Hűtés","","Névl.","kW","2.79 (3), 1.71 (4)","3.56 (3), 2.17 (4)","4.06 (3), 2.51 (4)"]
["","Fűtés","","Névl.","kW","1.91 (1), 2.43 (2)","2.18 (1), 2.68 (2)","2.46 (1), 3.42 (2)"]
["COP","","","","","4.91 (1), 3.71 (2)","4.83 (1), 3.66 (2)","4.87 (1), 3.64 (2)"]
["EER","","","","","3.35 (3), 5.34 (4)","3.26 (3), 5.31 (4)","3.16 (3), 5.04 (4)"]
["Méretek","Egység","","Magasság","mm","870","870","870"]
["","","","Szélesség","mm","1380","1380","1380"]
["","","","Mélység","mm","460","460","460"]
["Tömeg","Egység","","","kg","149","149","149"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","48.0","55.8","70.4"]
["","","Hűtés","Magas","m³/perc","63.1","70.4","85.0"]
["Üzemi tartomány","Fűtés","Vízoldal","Min.","°C","15 (6)","15 (6)","15 (6)"]
["","","","Max.","°C","60 (6)","60 (6)","60 (6)"]
["","Hűtés","Környezeti","Min.","°C száraz hőm.","10","10","10"]
["","","","Max.","°C száraz hőm.","43","43","43"]
["","","Vízoldal","Min.","°C","5","5","5"]
["","","","Max.","°C","22","22","22"]
["","Használati meleg víz","Környezeti","Min.","°C száraz hőm.","-25","-25","-25"]
["","","","Max.","°C száraz hőm.","35","35","35"]
["","","Vízoldal","Min.","°C","25","25","25"]
["","","","Max.","°C","55 (6)","55 (6)","55 (6)"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Töltet","","","kg","3.80","3.80","3.80"]
["","Töltet","","","tCO2Eq","2.57","2.57","2.57"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","3.44","3.37","3.42"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A++","A++","A++"]
["","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","4.82","4.73","4.70"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++","A+++","A+++"]
["Energiatakarékossági besorolás","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Kompresszor alkatrész","Fő áramellátás","","Fázis","","1~","1~","1~"]
["","","","Feszültség","V","230","230","230"]
["Áramellátás","Megnevezés","","","","V3","V3","V3"]
["","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","230","230","230"]
["Notes","","","","","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(2) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(2) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)"]
["","","","","","(3) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm.","(3) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm.","(3) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm."]
["","","","","","(4) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm.","(4) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm.","(4) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm."]
["","","","","","(5) - Az EN14825 szabvány szerint","(5) - Az EN14825 szabvány szerint","(5) - Az EN14825 szabvány szerint"]
["","","","","","(6) - További részleteket lásd az üzemi tartomány ábrán","(6) - További részleteket lásd az üzemi tartomány ábrán","(6) - További részleteket lásd az üzemi tartomány ábrán"]
["","","","","","(7) - A üzemelési módtól függ, lásd az összeszerelési kézikönyvet.","(7) - A üzemelési módtól függ, lásd az összeszerelési kézikönyvet.","(7) - A üzemelési módtól függ, lásd az összeszerelési kézikönyvet."]