{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSH-D / ERLA-DW17"]
[]
[]
[]
[]
["","","","","","EBSH16P30DF / ERLA16D2W17","EBSH16P50DF / ERLA16D2W17","EBSH16P30DF / ERLA16DAW17","EBSH16P50DF / ERLA16DAW17"]
["Beltéri egység","","","","","EBSH16P30DF","EBSH16P50DF","EBSH16P30DF","EBSH16P50DF"]
["Fűtőkapacitás","Névl.","","","kW","16.0 (1)","16.0 (1)","16.0 (1)","16.0 (1)"]
["Elektromos bemenet","Fűtés","","Névl.","kW","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)"]
["COP","","","","","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","L","XL","L","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","A+","A+","A+","A+"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","3.32","3.32","3.32","3.32"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A++","A++","A++","A++"]
["","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","4.61","4.61","4.61","4.61"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]