{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Hangnyomás szint","Névl.","","","dBA","32.0 (6)"]
["Refrigerant","GWP","","","","2,090"]
["","Feltöltés","","","kg","1.80"]
["","Type","","","","R-410A"]
["Üzemi tartomány","Beszerelési hely","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Fűtés","Vízoldal","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Tengervíz oldal","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Használati meleg víz","Vízoldal","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Elektromos bemenet","Névl.","","","kW","2.38 (1), 2.89 (2)"]
["Hangteljesítmény szintje","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Befoglaló méretek","Berendezés","","Szélesség","mm","600"]
["","","","Mélység","mm","728"]
["","","","Magasság","mm","1,730"]
["Casing","Material","","","","Előbevonattal ellátott fémlemez"]
["","Szín","","","","Fehér"]
["Tartály","Vízmennyiség","","","l","180"]
["","Korrózióvédelem","","","","Anód"]
["","Szigetelés","","Hőveszteség","kWó/24ó","1.36 (4)"]
["Súly","Berendezés","","","kg","210"]
["Felületfűtés","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","ηs (Szezonális felületfűtési hatékonyság)","%","194"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++"]
["","","","SCOP","","5.06"]
["","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","Seasonal space heating eff. class","","A++"]
["","","","ηs (Szezonális felületfűtési hatékonyság)","%","139"]
["","","","SCOP","","3.68"]
["Fűtőkapacitás","Névl.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Fázis","","","","3~"]
["","Név","","","","9W"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","400"]
["áramerősség","Javasolt biztosítékok","","","A","25"]
["Notes","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)"]
["","","","","","(3) - 40% propilén-glikollal"]
["","","","","","(4) - Az EN12897 szerinti hőveszteség"]
["","","","","","(5) - Beleértve a vezetékeket + lemezes hőcserélőt + tartalék hűtőt; kivéve a tágulási tartályt"]
["","","","","","(6) - A hangnyomás szintjét mikrofonnal mérik 1m távolságra az egységtől. Ez egy relatív érték a távolságtól és az akusztikus környezettől függően."]
["","","","","","(7) - Hőszivattyúval"]
["","","","","","(8) - Hőszivattyúval + tartalék fűtőelem"]
["","","","","","(9) - Tartalék fűtőelemmel"]