{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-D3"]
[]
[]
[]
[]
["","","","","","EHSHB04P30DA3","EHSHB08P30DA3","EHSHB08P50DA3"]
["Burkolat","Szín","","","","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)"]
["","Anyag","","","","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén"]
["Méretek","Egység","","Magasság","mm","1891","1891","1896"]
["","","","Szélesség","mm","595","595","790"]
["","","","Mélység","mm","615","615","790"]
["Tömeg","Egység","","","kg","76.0","76.0","99.0"]
["PED","Kategória","","","","cikk 3,3","cikk 3,3","cikk 3,3"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Töltet","","","kg","1.50","1.50","1.50"]
["Hangteljesítmény szintje","Névl.","","","dB(A)","39","39","39"]
["Üzemi tartomány","Fűtés","Vízoldal","Min.","°C","18","18","18"]
["","","","Max.","°C","65","65","65"]
["","Hűtés","Környezeti","Min.","°C száraz hőm.","10","10","10"]
["","","Vízoldal","Min.","°C","5","5","5"]
["","","","Max.","°C","22","22","22"]
["Áramellátás","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","230","230","230"]
["Elektromos fűtő","Áramellátás","","Név","","3V / 9W","3V / 9W","3V / 9W"]
["","","","Fázis","","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frekvencia","Hz","50","50","50"]
["Notes","","","","","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]
["","","","","","","","(5) - A tartály felmelegítése csak hőszivattyúval, elektromos fűtőelem nélkül"]