{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-E"]
[]
[]
[]
[]
["","","","","","EHSXB04P30EF","EHSXB04P50EF","EHSXB04P50EG","EHSXB04P30EG","EHSXB08P30EF","EHSXB08P50EF","EHSXB08P50EG","EHSXB08P30EG"]
["Burkolat","Szín","","","","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)"]
["","Anyag","","","","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén"]
["Méretek","Egység","","Magasság","mm","1,892","1,905","1,910","1,891","1,892","1,905","1,910","1,891"]
["","","","Szélesség","mm","594","792","792","594","594","792","792","594"]
["","","","Mélység","mm","644","812","817","644","644","812","817","644"]
["Tömeg","Egység","","","kg","79","110","104","80.0","79","110","104","80.0"]
["PED","Kategória","","","","4.3 cikk","4.3 cikk","4.3 cikk","4.3 cikk","4.3 cikk","4.3 cikk","4.3 cikk","4.3 cikk"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675","675.0","675.0","675","675","675.0","675.0"]
["","Töltet","","","kg","1.5","1.5","1.50","1.50","1.5","1.5","1.50","1.50"]
["Hangteljesítmény szintje","Névl.","","","dB(A)","39","39","39","39","39","39","39","39"]
["Üzemi tartomány","Fűtés","Vízoldal","Min.","°C","18","18","18","18","18","18","18","18"]
["","","","Max.","°C","65","65","65","65","65","65","65","65"]
["","Hűtés","Környezeti","Min.","°C száraz hőm.","10","10","10","10","10","10","10","10"]
["","","Vízoldal","Min.","°C","5","5","5","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22","22","22","22"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","50","50","50"]
["","Feszültség","","","V","230","230","230","230","230","230","230","230"]
["Notes","","","","","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség"]