{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-E6V / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHVH08S18EA6V / ERGA06EAV3H","EHVH08S18EJ6V / ERGA06EAV3H","EHVH08S23EA6V / ERGA06EAV3H","EHVH08S23EJ6V / ERGA06EAV3H"]
["Fűtőkapacitás","Névl.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)"]
["Elektromos bemenet","Fűtés","","Névl.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["Áramfelvétel","Háztartási melegvíz 10°C és 50°C között","","Névl.","kWh","2.48","2.48","3.01","3.01"]
["Felmelegedési idő 10°C-ról 50°C-ra","ó","","","","1 óra 28 perc","1 óra 28 perc","1 óra 40 perc","1 óra 40 perc"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","L","L","XL","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","A+","A+","A+","A+"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","3.26","3.26","3.26","3.26"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A++","A++","A++","A++"]
["","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","4.47","4.47","4.47","4.47"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++","A+++","A+++","A+++"]
["Energiatakarékossági besorolás","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]