{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E3V / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHVX04S23EJ3V / ERGA04EAV37","EHVX04S18EA3V / ERGA04EAV37","EHVX04S18EJ3V / ERGA04EAV37","EHVX04S23EA3V / ERGA04EAV37"]
["Fűtőkapacitás","Névl.","","","kW","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)"]
["Hűtési teljesítmény","Névl.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["Elektromos bemenet","Fűtés","","Névl.","kW","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)"]
["","Hűtés","","Névl.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["Áramfelvétel","Háztartási melegvíz 10°C és 50°C között","","Névl.","kWh","3.01","2.48","2.48","3.01"]
["Felmelegedési idő 10°C-ról 50°C-ra","ó","","","","1 óra 40 perc","1 óra 28 perc","1 óra 28 perc","1 óra 40 perc"]
["COP","","","","","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","XL","L","L","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","A","A","A","A"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","3.29","3.29","3.29","3.29"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A++","A++","A++","A++"]
["","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","4.96","4.96","4.96","4.96"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++","A+++","A+++","A+++"]
["Energiatakarékossági besorolás","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]