{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":13,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E9W / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHVX08S18EA9W / ERGA06EAV3A","EHVX08S23EA9W / ERGA06EAV3A","EHVX08S18EJ9W / ERGA06EAV3A","EHVX08S23EJ9W / ERGA06EAV3A","EHVX08S18EA9W / ERGA08EAV3A","EHVX08S23EA9W / ERGA08EAV3A","EHVX08S18EJ9W / ERGA08EAV3A","EHVX08S23EJ9W / ERGA08EAV3A"]
["Fűtőkapacitás","Névl.","","","kW","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)"]
["Hűtési teljesítmény","Névl.","","","kW","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)"]
["Elektromos bemenet","Fűtés","","Névl.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["","Hűtés","","Névl.","kW","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)"]
["Áramfelvétel","Háztartási melegvíz 10°C és 50°C között","","Névl.","kWh","2.48","3.01","2.48","3.01","2.48","3.01","2.48","3.01"]
["Felmelegedési idő 10°C-ról 50°C-ra","ó","","","","1 óra 28 perc","1 óra 40 perc","1 óra 28 perc","1 óra 40 perc","1 óra 28 perc","1 óra 40 perc","1 óra 28 perc","1 óra 40 perc"]
["COP","","","","","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)"]
["EER","","","","","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.4 (1), 3.14 (2)","5.4 (1), 3.14 (2)","5.4 (1), 3.14 (2)","5.4 (1), 3.14 (2)"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","L","XL","L","XL","L","XL","L","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","3.27","3.27","3.27","3.27","3.3","3.3","3.3","3.3"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","4.52","4.52","4.52","4.52","4.61","4.61","4.61","4.61"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]