{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","EHYHBH05AFV32","EHYHBH05AAV32","EHYHBH08AFV32","EHYHBH08AAV32"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér","Fehér"]
["","Anyag","","","","Előbevonattal ellátott fémlemez","Előbevonattal ellátott fémlemez","Előbevonattal ellátott fémlemez","Előbevonattal ellátott fémlemez"]
["Méretek","Egység","","Magasság","mm","902","902","902","902"]
["","","","Szélesség","mm","450","450","450","450"]
["","","","Mélység","mm","164","164","164","164"]
["Tömeg","Egység","","","kg","30.0","30.0","31.2","31.2"]
["PED","Kategória","","","","Cikk3§3, A 97/23/EK 3.6 fejezet 1. cikkelye alapján nem tartozik a PED kategóriába","Cikk3§3, A 97/23/EK 3.6 fejezet 1. cikkelye alapján nem tartozik a PED kategóriába","I. kategória","I. kategória"]
["Víz oldali hőcserélő","Vízáramlás aránya","Fűtés","Max.","l/perc","23.0 (7)","23.0","23.5 (7)","23.5"]
["Hangteljesítmény szintje","Névl.","","","dB(A)","42.0","42.0","42.0","42.0"]
["Üzemi tartomány","Fűtés","Vízoldal","Min.","°C","25 (8)","25","25 (8)","25"]
["","","","Max.","°C","55 (8)","55","55 (8)","55"]
["Áramellátás","Megnevezés","","","","V3","V3","V3","V3"]
["","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","230","230","230","230"]
["Vezeték csatlakozások","A felhasználói interfésszel való csatlakoztatásra","","Mennyiség","","2","2","2","2"]
["Vezetékcsatlakozások","A felhasználói interfésszel való csatlakoztatásra","","Megjegyzés","","0,75 mm² - 1,25 mm² (max hossz 500m)","0,75 mm² - 1,25 mm² (max hossz 500m)","0,75 mm² - 1,25 mm² (max hossz 500m)","0,75 mm² - 1,25 mm² (max hossz 500m)"]
["Notes","","","","","(1) - Csak a beltéri egységhez","","(1) - Csak a beltéri egységhez"]
["","","","","","(2) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 35 °C (Hőm. különbség = 5 °C), kazán kihagyva","","(2) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 35 °C (Hőm. különbség = 5 °C), kazán kihagyva"]
["","","","","","(3) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 45℃ (Hőm. különbség = 5 °C), kazán kihagyva","","(3) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 45℃ (Hőm. különbség = 5 °C), kazán kihagyva"]
["","","","","","(4) - Min. required","","(4) - Min. required"]
["","","","","","(5) - Kazán kihagyva","","(5) - Kazán kihagyva"]
["","","","","","(6) - A *HYHB* és *HYKOMB33AA működési tartományáról lásd a működési tartomány ábrát","","(6) - A *HYHB* és *HYKOMB33AA működési tartományáról lásd a működési tartomány ábrát"]