{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AAV3 / EVLQ08CAV3","EHYHBX08AFV3 / EVLQ08CAV3"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","A"]
["COP","","","","","4.45 (3), 3.42 (4)","4.45, 3.42"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","Seasonal space heating eff. class","","A++"]
["","","","ηs (Szezonális felületfűtési hatékonyság)","%","129"]
["","","","SCOP","","3.29"]
["Hűtési teljesítmény","Névl.","","","kW","6.86 (4), 5.36 (4)"]
["","Min.","","","kW","2.50 (3), 2.50 (4)"]
["EER","","","","","3.42 (3), 2.29 (4)","3.42, 2.29"]
["Fűtőkapacitás","Névl.","","","kW","7.40 (3), 6.89 (4)"]
["","Min.","","","kW","1.80 (3), 1.80 (4)"]
["","Max.","","","kW","10.0 (3), 9.53 (4)"]
["Áramfelvétel","Hűtés","","Névl.","kW","2.01 (3), 2.34 (4)"]
["","Fűtés","","Névl.","kW","1.66 (3), 2.01 (4)"]
["Notes","","","","","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(2) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["","","","","","(3) - 1. feltétel: hűtés Tkörny 35°C - LWE 18℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Tkörny 35 °C - LWE 7 °C (DT = 5 °C), vízmelegítő kihagyásával"]
["","","","","","(4) - 2. feltétel: hűtés Tkörny 35°C - LWE 7℃ (DT = 5°C); fűtés Tkörny DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(4) - Tkörny 35 °C - LWE 18℃ (DT = 5 °C), vízmelegítő kihagyásával"]
["","","","","","(5) - Tkörny 35 °C - LWE 7 °C (DT = 5 °C), vízmelegítő kihagyásával","(5) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 35 °C (Hőm. különbség = 5 °C), kazán kihagyva"]
["","","","","","(6) - Tkörny 35 °C - LWE 18℃ (DT = 5 °C), vízmelegítő kihagyásával","(6) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 45℃ (Hőm. különbség = 5 °C), kazán kihagyva"]
["","","","","","(7) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 35 °C (Hőm. különbség = 5 °C), kazán kihagyva"]
["","","","","","(8) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 45℃ (Hőm. különbség = 5 °C), kazán kihagyva"]
["Fűtőkapacitás","Min.","","","kW","","1.80, 1.80"]
["","Névl.","","","kW","","7.40, 6.89"]
["","Max.","","","kW","","10.0, 9.53"]
["Hűtési teljesítmény","Min.","","","kW","","2.50, 2.50"]
["","Névl.","","","kW","","6.86, 5.36"]
["Elektromos bemenet","Fűtés","","Névl.","kW","","1.66, 2.01"]
["","Hűtés","","Névl.","kW","","2.01, 2.34"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","","A"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","","3.29"]
["","","","Szezonális felületfűtési hatékonysági osztály","","","A++"]
["","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","","4.28"]
["","","","Szezonális felületfűtési hatékonysági osztály","","","A++"]
["Energiatakarékossági besorolás","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]