{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Burkolat","Szín","","","","Fehér"]
["","Anyag","","","","Előbevonattal ellátott fémlemez"]
["Méretek","Egység","","Magasság","mm","902"]
["","","","Szélesség","mm","450"]
["","","","Mélység","mm","164"]
["Tömeg","Egység","","","kg","31.2"]
["PED","Kategória","","","","I. kategória"]
["Víz oldali hőcserélő","Vízáramlás aránya","Fűtés","Max.","l/perc","23.5 (7)"]
["Hangteljesítmény szintje","Névl.","","","dB(A)","42.0"]
["Üzemi tartomány","Fűtés","Vízoldal","Min.","°C","25 (8)"]
["","","","Max.","°C","55 (8)"]
["","Hűtés","Környezeti","Min.","°C száraz hőm.","10 (8)"]
["","","Vízoldal","Min.","°C","5 (8)"]
["","","","Max.","°C","22 (8)"]
["Áramellátás","Megnevezés","","","","V3"]
["","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","230"]
["Vezeték csatlakozások","A felhasználói interfésszel való csatlakoztatásra","","Mennyiség","","2"]
["Vezetékcsatlakozások","A felhasználói interfésszel való csatlakoztatásra","","Megjegyzés","","0,75 mm² - 1,25 mm² (max hossz 500m)"]
["Notes","","","","","(1) - Csak a beltéri egységhez"]
["","","","","","(2) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 35 °C (Hőm. különbség = 5 °C), kazán kihagyva"]
["","","","","","(3) - Száraz hőm./nedves hőm. 7 °C / 6 °C - T(előremenő) 45℃ (Hőm. különbség = 5 °C), kazán kihagyva"]
["","","","","","(4) - Tkörny 35 °C - LWE 7 °C (DT = 5 °C), vízmelegítő kihagyásával"]
["","","","","","(5) - Tkörny 35 °C - LWE 18℃ (DT = 5 °C), vízmelegítő kihagyásával"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Kazán kihagyva"]
["","","","","","(8) - A *HYHB* és *HYKOMB33AA működési tartományáról lásd a működési tartomány ábrát"]