{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYKOMB-AA3"]
[]
[]
[]
[]
["","","","","","EHYKOMB33AA3"]
["Gáz","Csatlakozás","","Átmérő","mm","15"]
["","Fogyasztás (G20)","","perc","m³/ó","0.79"]
["","","","Max.","m³/ó","3.39"]
["","Fogyasztás (G25)","","perc","m³/ó","0.89"]
["","","","Max.","m³/ó","3.92"]
["","Fogyasztás (G31)","","perc","m³/ó","0.30"]
["","","","Max.","m³/ó","1.29"]
["","NOx osztály","","","","6"]
["","NOx szint (G20)","","","mg/kWh","36"]
["Központi fűtés","Hőleadási teljesítmény Qn (nettó fűtőérték)","Névl.","Min.","kW","7.6"]
["","","","Max.","kW","27.0"]
["","Hőleadási teljesítmény Qn (bruttó fűtőérték)","Névl.","Min.","kW","8.4"]
["","","","Max.","kW","30.0"]
["","Teljesítmény Pn 80/60°C-on","","Min.","kW","7.5"]
["","","","Névl.","kW","26.6"]
["","Teljesítmény Pn 37/30°C-on","","Névl.","kW","8.2"]
["","Víz hőmérséklet","","Max.","°C","90"]
["Használati melegvíz","Felvételi teljesítmény Qnw (nettó fűtőérték)","Névl.","Min.","kW","7.6"]
["","","","Max.","kW","32.7"]
["","Felvételi teljesítmény Qnw (bruttó fűtőérték)","Névl.","Min.","kW","8.4"]
["","","","Max.","kW","36.3"]
["","Komfort osztály (EN13203)","","","","XL"]
["","Hőmérséklet","","Max.","°C","65"]
["Befúvott levegő","Koncentrikus","","","","Nem"]
["Füstgáz","Hőmérséklet","","Max.","°C","70"]
["","Csatlakozás","","","mm","60"]
["","Átfolyási tömeg (G20)","","Max.","kg/h","54.4"]
["","Átfolyási tömeg (G25)","","Max.","kg/h","54.4"]
["","Átfolyási tömeg (G31)","","Max.","kg/h","53.6"]
["Burkolat","Szín","","","","RAL9010"]
["","Anyag","","","","Előbevonattal ellátott fémlemez"]
["Méretek","Berendezés","Magasság","Burkolat","mm","710"]
["","Egység","","Szélesség","mm","450"]
["","","","Mélység","mm","240"]
["Súly","Berendezés","","Üres","kg","36"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","XL"]
["","","","Vízmelegítési hatékonysági osztály","","A"]
["Felületfűtés","Általános","","Szezonális felületfűtés hatékonysági osztály","","A"]